#!/bin/sh
###############################################################################
#                                                                             #
# IPFire.org - A linux based firewall                                         #
# Copyright (C) 2007-2022  IPFire Team  <info@ipfire.org>                     #
#                                                                             #
# This program is free software: you can redistribute it and/or modify        #
# it under the terms of the GNU General Public License as published by        #
# the Free Software Foundation, either version 3 of the License, or           #
# (at your option) any later version.                                         #
#                                                                             #
# This program is distributed in the hope that it will be useful,             #
# but WITHOUT ANY WARRANTY; without even the implied warranty of              #
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the               #
# GNU General Public License for more details.                                #
#                                                                             #
# You should have received a copy of the GNU General Public License           #
# along with this program.  If not, see <http://www.gnu.org/licenses/>.       #
#                                                                             #
###############################################################################

. /etc/sysconfig/rc
. ${rc_functions}
. /etc/init.d/networking/functions.network

#Define some defaults
INET_VLAN=7
IPTV_VLAN=8
ATM_DEV=0

eval $(/usr/local/bin/readhash /var/ipfire/main/settings)
if [ "$RRDLOG" == "" ]; then
	RRDLOG=/var/log/rrd
fi

eval $(/usr/local/bin/readhash /var/ipfire/ethernet/settings)
eval $(/usr/local/bin/readhash /var/ipfire/dns/settings)
eval $(/usr/local/bin/readhash /var/ipfire/mac/settings)

MAC=$(tr - : <<<$MAC)
MAC1=$(tr - : <<<$MAC1)
MAC2=$(tr - : <<<$MAC2)

TYPE="${RED_TYPE}"
DEVICE="${RED_DEV}"

if [ "$TYPE" == "STATIC" ] || [ "$TYPE" == "DHCP" ]; then
	if [ "$DEVICE" == "" ]; then
		boot_mesg "No device for red network. Please run setup." ${FAILURE}
		echo_failure
		[ "${1}" == "start" ] && exit 0
	fi
fi

if [ "${TYPE}" == "STATIC" ]; then
	if [ "${DEVICE}" != "${GREEN_DEV}" ]; then
		ADDRESS="${RED_ADDRESS}"
		NETADDRESS="${RED_NETADDRESS}"
		NETMASK="${RED_NETMASK}"
		MTU="${RED_MTU}"
	else
		ADDRESS="${GREEN_ADDRESS}"
		NETADDRESS="${GREEN_NETADDRESS}"
		NETMASK="${GREEN_NETMASK}"
		MTU="${GREEN_MTU}"
	fi
	GATEWAY="${DEFAULT_GATEWAY}"
	# DNS1
	# DNS2

	if [ -n "${ADDRESS}" -a -n "${NETMASK}" ]; then
		PREFIX=`whatmask ${NETMASK} | grep -e ^CIDR | awk -F': ' '{ print $2 }' | cut -c 2-`
		args="${args} ${ADDRESS}/${PREFIX}"
	else
		boot_mesg "ADDRESS and/or NETMASK variable missing from input, cannot continue." ${FAILURE}
		echo_failure
		exit 1
	fi
fi

case "${1}" in
	start)
		if [ "${DEVICE}" != "${GREEN_DEV}" ] && [ "${DEVICE}" != "" ]; then
			boot_mesg "Bringing up the ${DEVICE} interface..."
			boot_mesg_flush
			# Check if an interface is there...
			if ip link show ${DEVICE} > /dev/null 2>&1; then
				link_status=`ip link show ${DEVICE} 2> /dev/null`
				if [ -n "${link_status}" ]; then
					if ! echo "${link_status}" | grep -q UP; then
						if [ -n "$MAC" ]; then
							boot_mesg "Setting mac address on ${DEVICE} to ${MAC}"
							ip link set dev ${DEVICE} address ${MAC}
							evaluate_retval
						fi
						ip link set ${DEVICE} up
					fi
				fi
			else
				boot_mesg "Interface ${DEVICE} doesn't exist." ${FAILURE}
				echo_failure
				exit 1
			fi
		fi

		if [ "${TYPE}" == "STATIC" ]; then
			# Set the MTU
			if [ -n "${MTU}" ]; then
				if ! ip link set dev "${DEVICE}" mtu "${MTU}" &>/dev/null; then
					boot_mesg "Could not set MTU of ${MTU} to ${DEVICE}..."
					echo_warning
				fi
			fi

			if [ "$DEVICE" != "${GREEN_DEV}" ]; then
				boot_mesg "Adding IPv4 address ${ADDRESS} to the ${DEVICE} interface..."
				ip addr add ${args} dev ${DEVICE}
				evaluate_retval
			fi
			echo -n "${DEVICE}" > /var/ipfire/red/iface
			echo -n "${ADDRESS}"  > /var/ipfire/red/local-ipaddress
			echo -n "${GATEWAY}" > /var/ipfire/red/remote-ipaddress
			grep -v -E "\<gateway\>" /etc/hosts > /tmp/hosts
			echo "$GATEWAY	gateway"  >> /tmp/hosts
			mv /tmp/hosts /etc/hosts
			touch /var/ipfire/red/active

			# Create route to default gateway
			ip route add ${GATEWAY} dev ${DEVICE}

			boot_mesg "Setting up default gateway ${GATEWAY}..."
			ip route add default via ${GATEWAY} dev ${DEVICE}
			evaluate_retval

			if [ -d "/sys/class/net/${DEVICE}" ]; then
				# has carrier ?
				if [ ! "$(</sys/class/net/${DEVICE}/carrier)" = "1" ]; then
					boot_mesg -n "Wait for carrier on ${DEVICE} "
					for (( i=30; i>1; i-- )) do
						if [ "$(</sys/class/net/${DEVICE}/carrier)" = "1" ]; then
							break;
						fi
						boot_mesg -n "."
						sleep 2
					done
					boot_mesg ""
					if [ ! "$(</sys/class/net/${DEVICE}/carrier)" = "1" ]; then
						echo_failure
					else
						echo_ok
					fi
				fi
			fi

			run_subdir ${rc_base}/init.d/networking/red.up/

			# Configure aliases only if red static
			/usr/local/bin/setaliases

		elif [ "${TYPE}" == "DHCP" ]; then
			# Add firewall rules to allow comunication with the dhcp server on red.
			iptables -A REDINPUT -p tcp --source-port 67 --destination-port 68 -i ${DEVICE} -j ACCEPT
			iptables -A REDINPUT -p udp --source-port 67 --destination-port 68 -i ${DEVICE} -j ACCEPT

			echo -n "${DEVICE}" > /var/ipfire/red/iface

			# Check if the wlan-client is used on red.
			# To determine this we check if a wpa_supplicant is running.
			pid="$(pidof wpa_supplicant)"

			if [ -z "${pid}" ]; then
				# No wpa_supplicant is running. So it's save to start dhcpcd.
				dhcpcd_start "${DEVICE}"
			fi

		elif [ "$TYPE" == "PPPOE" ]; then

			if ( ps ax | grep -q [p]ppd ); then 
			    boot_mesg "pppd is still running." ${FAILURE}
			    echo_failure
			    exit 1
			fi

			eval $(/usr/local/bin/readhash /var/ipfire/ppp/settings)

			[ -c "/dev/ppp" ] || mknod /dev/ppp c 108 0

			# We force the plugin method, anyway.
			METHOD="PPPOE_PLUGIN"

			PPP_NIC=${DEVICE}

			if [ "$TYPE" == "pppoeatm" ] || [ "$TYPE" == "pptpatm" ]; then
				PPP_NIC=nas${ATM_DEV}
				DEVICE=nas${ATM_DEV}
				boot_mesg "Creating ATM-Bridge as $PPP_NIC ..."
				br2684ctl -c${ATM_DEV} -e${ENCAP} -a${ATM_DEV}.${VPI}.${VCI} >/dev/null 2>&1 &
				sleep 1

				# use user-defined or green mac address for nas0
				if [ -n "$MAC" ]; then
					ip link set dev nas${ATM_DEV} address ${MAC}
				else
					ip link set dev nas${ATM_DEV} address $(cat /sys/class/net/green0/address)
				fi

				if [ "$TYPE" == "pppoeatm" ]; then
					TYPE="pppoe"
				fi
				if [ "$TYPE" == "pptpatm" ]; then
					TYPE="pptp"
				fi

			# QMI
			elif [ "$TYPE" = "qmi" ]; then
				DEVICE="$(qmi_find_device "${RED_DEV}")"

				boot_mesg "Bringing up QMI on ${RED_DEV} (${DEVICE})..."

				# Enable RAW-IP mode
				qmi_enable_rawip_mode "${RED_DEV}"

				# Configure APN
				qmi_configure_apn "${DEVICE}" "${APN}" "${AUTH}" "${USERNAME}" "${PASSWORD}"

				# Set up the interface
				ip link set "${RED_DEV}" up &>/dev/null

				# Write red device name to the corresponding file.
				echo -n "${RED_DEV}" > /var/ipfire/red/iface

				# Start the DHCP client
				dhcpcd_start "${RED_DEV}" --dhcp

				# Done
				exit 0
			fi

			if [ "$TYPE" == "vdsl" ]; then
				boot_mesg "Creating VLAN Interface ${DEVICE}.${INET_VLAN} ..."
				modprobe 8021q
				vconfig add ${DEVICE} ${INET_VLAN}
				if [ -n "$MAC1" ]; then
					boot_mesg "Setting mac address on ${DEVICE}.${INET_VLAN} to ${MAC1}"	
					ip link set dev ${DEVICE}.${INET_VLAN} address ${MAC1}
					evaluate_retval
				fi
				PPP_NIC=${DEVICE}.${INET_VLAN}
				sleep 0.2
				ip link set ${PPP_NIC} up
				TYPE="pppoe"
			fi
			if [ "${IPTV}" == "enable" ]; then
				PIDFILE="/var/run/dhcpcd/${DEVICE}.${IPTV_VLAN}.pid"
				LEASEINFO="/var/ipfire/dhcpc/dhcpcd-${DEVICE}.${IPTV_VLAN}.info"
				# Test to see if there is a stale pid file
				if [ -f "$PIDFILE" ]; then
					ps `cat "$PIDFILE"` | grep dhcpcd > /dev/null
					if [ $? != 0 ]; then
						rm -f /var/run/dhcpcd/${DEVICE}.${IPTV_VLAN}.pid > /dev/null
					fi
				fi

				if [ ! -f "$PIDFILE" ]; then
					boot_mesg "Creating VLAN Interface ${DEVICE}.${IPTV_VLAN} ..."
					modprobe 8021q
					vconfig add ${DEVICE} ${IPTV_VLAN}
					if [ -n "$MAC2" ]; then
						boot_mesg "Setting mac address on ${DEVICE}.${IPTV_VLAN} to ${MAC2}"
						ip link set dev ${DEVICE}.${IPTV_VLAN} address ${MAC2}
						evaluate_retval
					fi
					boot_mesg -n "Starting dhcpcd on the ${DEVICE}.${IPTV_VLAN} interface..."
					/sbin/dhcpcd ${DEVICE}.${IPTV_VLAN} ${DHCP_START} >/dev/null 2>&1
					RET="$?"

					if [ "$RET" = "0" ]; then
						. /var/ipfire/dhcpc/dhcpcd-${DEVICE}.${IPTV_VLAN}.info
						echo ""
						echo_ok
						boot_mesg "           DHCP Assigned Settings for ${DEVICE}.${IPTV_VLAN}:"
						boot_mesg_flush
						boot_mesg "           IP Address:      $ip_address"
						boot_mesg_flush
						boot_mesg "           Hostname:        $RED_DHCP_HOSTNAME"
						boot_mesg_flush
						boot_mesg "           Subnet Mask:     $subnet_mask"
						boot_mesg_flush
						boot_mesg "           Default Gateway: $routers"
						boot_mesg_flush
						boot_mesg "           DNS Server:      $domain_name_servers"
						boot_mesg_flush

					else
						echo ""
						$(exit "$RET")
						evaluate_retval
					fi
				fi
			fi
			if [ "$TYPE" == "pppoe" ] || [ "$TYPE" == "pptp" ]; then
				if [ "$PPP_NIC" == "" ]; then
					boot_mesg "No device for red interface given. Check netsetup or dialprofile!" ${FAILURE}
					echo_failure
					exit 0
				fi
				boot_mesg "Bringing up the $TYPE interface on $PPP_NIC ..."
				ip addr flush dev $PPP_NIC >/dev/null 2>&1
				if [ "$TYPE" == "pptp" ]; then
					if [ "$PPTP_NICCFG" == "dhcp" ]; then
						# Test to see if there is a stale pid file
						if [ -f "$PIDFILE" ]; then
							ps `cat "$PIDFILE"` | grep dhcpcd > /dev/null
							if [ $? != 0 ]; then
								rm -f /var/run/dhcpcd/${DEVICE}.pid > /dev/null
							fi
						fi

						if [ ! -f "$PIDFILE" ]; then
							boot_mesg -n "Starting dhcpcd on the ${DEVICE} interface..."
							/sbin/dhcpcd ${DEVICE} ${DHCP_START} >/dev/null 2>&1
							RET="$?"

							if [ "$RET" = "0" ]; then
								. /var/ipfire/dhcpc/dhcpcd-${DEVICE}.info
								echo ""
								echo_ok
								boot_mesg "           DHCP Assigned Settings for ${DEVICE}:"
								boot_mesg_flush
								boot_mesg "           IP Address:      $ip_address"
								boot_mesg_flush
								boot_mesg "           Hostname:        $RED_DHCP_HOSTNAME"
								boot_mesg_flush
								boot_mesg "           Subnet Mask:     $subnet_mask"
								boot_mesg_flush
								boot_mesg "           Default Gateway: $routers"
								boot_mesg_flush
								boot_mesg "           DNS Server:      $domain_name_servers"
								boot_mesg_flush
								/sbin/route add $PPTP_PEER gw $routers $PPP_NIC
							else
								echo ""
								$(exit "$RET")
								evaluate_retval
							fi
						fi
					else
						ip addr add $PPTP_NICCFG dev $PPP_NIC
					fi
				fi
				ip link set ${PPP_NIC} up
				if [ -n "${PPTP_ROUTE}" ]; then
					boot_mesg "Set route ${PPTP_ROUTE} to pptp server..."
					route add ${PPTP_ROUTE}
				fi
			else
				boot_mesg "Bringing up the PPP via ${TYPE} on ${COMPORT}..."
			fi

			###                      ###
			### Configuring the pppd ###
			###                      ###

			### Plugin Options
			#
			if [ "$TYPE" == "pppoe" ]; then
				[ "${METHOD}" == "PPPOE_PLUGIN" ] && \
					PLUGOPTS="plugin rp-pppoe.so"
			fi

			### Synchronous Mode
			#
			#PPPOE_SYNC=-s
			#PPPD_SYNC=sync

			### Access Concentrator Name
			#
			if [ -n "${CONCENTRATORNAME}" ]; then
				ACNAME="-C ${CONCENTRATORNAME}"
			fi

			### Service Name
			#
			if [ -n "${SERVICENAME}" ]; then
				if [ "${METHOD}" == "PPPOE_PLUGIN" ]; then
					PLUGOPTS+=" rp_pppoe_service ${SERVICENAME}"
				else
					SERVICENAME="-S ${SERVICENAME}"
				fi
			fi

			### Authentication Types
			#
			if [ "${AUTH}" == "pap" ]; then
				AUTH="-chap"
			elif [ "${AUTH}" == "chap" ]; then
				AUTH="-pap"
			else
				AUTH=""
			fi

			### Dial On Demand
			#
			if [ "${RECONNECTION}" != "persistent" ]; then
				if [ "${TIMEOUT}" != "0" ] && [ "${TIMEOUT}" != "" ]; then
					SECONDS=$[${TIMEOUT} * 60]
				else
					SECONDS=300
				fi
				if [ "${RECONNECTION}" == "dialondemand" ]; then
					touch /var/ipfire/red/dial-on-demand
					DEMAND="demand persist idle ${SECONDS} 10.112.112.112:10.112.112.113"
					DEMAND+=" ipcp-accept-remote ipcp-accept-local noipdefault ktune"
				fi
			fi

			if [ "$TYPE" == "pppoe" ]; then
				### When using pppoe-plugin the device has to be the last option
				#
				[ "${METHOD}" == "PPPOE_PLUGIN" ] && PLUGOPTS+=" $PPP_NIC"
			fi

			if [ "$TYPE" == "modem" ]; then
				PLUGOPTS=" /dev/${COMPORT} ${DTERATE} connect /etc/ppp/dialer lock modem crtscts"
				METHOD="PPPOE_PLUGIN"
			elif [ "$TYPE" == "serial" ]; then
				PLUGOPTS=" /dev/${COMPORT} ${DTERATE} connect /bin/true lock modem crtscts"
				METHOD="PPPOE_PLUGIN"
			fi

			### Standard PPP options we always use
			#
			PPP_STD_OPTIONS="$PLUGOPTS usepeerdns defaultroute noipdefault noauth"
			PPP_STD_OPTIONS+=" default-asyncmap hide-password nodetach noipv6"
			PPP_STD_OPTIONS+=" noaccomp nodeflate nopcomp novj novjccomp"
			PPP_STD_OPTIONS+=" nobsdcomp user ${USERNAME} lcp-echo-interval 20"
			PPP_STD_OPTIONS+=" lcp-echo-failure 5 ${AUTH}"

			if [ -n "${MTU}" ]; then
				PPP_STD_OPTIONS="${PPP_STD_OPTIONS} mtu ${MTU}"
			fi

			if [ -n "${MRU}" ]; then
				PPP_STD_OPTIONS="${PPP_STD_OPTIONS} mru ${MRU}"
			fi

			### Debugging
			#
			if [ "${DEBUG}" == "on" ]; then
				DEBUG="debug"
			else
				DEBUG=""
			fi

			### PPPoE invocation
			#
			if [ "$TYPE" == "pppoe" ]; then
				PPPOE_CMD="/usr/sbin/pppoe -p /var/run/ppp-ipfire.pid.pppoe -I $PPP_NIC"
				PPPOE_CMD+=" -T 80 -U $PPPOE_SYNC $ACNAME $SERVICENAMEOPT"
			fi

			### PPTP ###
			#
			if [ "$TYPE" == "pptp" ]; then
				PPPOE_CMD="pptp $PPTP_PEER --nolaunchpppd"
				METHOD=""
			fi

			### Run everything
			#
			if [ "$METHOD" == "PPPOE_PLUGIN" ]; then
				/usr/sbin/pppd $PPP_STD_OPTIONS $DEBUG $DEMAND >/dev/null 2>&1 &
				evaluate_retval
				# echo PLUGIN: /usr/sbin/pppd $PPP_STD_OPTIONS $DEBUG $DEMAND
			else
				/usr/sbin/pppd pty "$PPPOE_CMD" $PPP_STD_OPTIONS $DEBUG $DEMAND $PPPD_SYNC >/dev/null 2>&1 &
				evaluate_retval
				# echo PPP: /usr/sbin/pppd pty "$PPPOE_CMD" $PPP_STD_OPTIONS $DEBUG $DEMAND $PPPD_SYNC
			fi

			/etc/rc.d/init.d/connectd start
			# Add a NaN value to ppp0 rrd to supress spikes at reconnect
			rrdtool update $RRDLOG/collectd/localhost/interface/if_octets-ppp0.rrd \
				$(date +%s):: > /dev/null 2>&1
			exit 0
		fi
		;;

	stop)
		rm -f /var/ipfire/red/{active,device,dial-on-demand,dns1,dns2,local-ipaddress,remote-ipaddress,resolv.conf}

		if [ "$TYPE" == "STATIC" ]; then
			boot_mesg "Stopping default gateway ${GATEWAY}..."
			ip route del default via ${GATEWAY} >/dev/null 2>&1
			echo_ok
			if [ "$DEVICE" != "${GREEN_DEV}" ]; then
				boot_mesg "Removing IPv4 addresses from the ${DEVICE} interface..."
				ip addr flush dev ${DEVICE}
				evaluate_retval
			fi
			run_subdir ${rc_base}/init.d/networking/red.down/

		elif [ "$TYPE" == "PPPOE" ]; then
			eval $(/usr/local/bin/readhash /var/ipfire/ppp/settings)

			if [ "${TYPE}" = "qmi" ]; then
				boot_mesg "Bringing down the QMI interface ${RED_DEV}..."
				DEVICE="$(qmi_find_device "${RED_DEV}")"

				# Stop the DHCP client on RED
				dhcpcd_stop "${RED_DEV}"

				# Reset any QMI settings
				qmi_reset "${DEVICE}"

				exit 0
			fi

			boot_mesg "Bringing down the PPP interface ..."
			rm -f /var/ipfire/red/keepconnected
			killall -w -s TERM /usr/sbin/pppd 2>/dev/null
			evaluate_retval
			# Add a NaN value to ppp0 rrd to supress spikes at reconnect
			rrdtool update $RRDLOG/collectd/localhost/interface/if_octets-ppp0.rrd \
				$(date +%s):: > /dev/null 2>&1

		elif [ "$TYPE" == "DHCP" ]; then
			# Check if the wlan-client is used on red.
                        # To determine this we check if a wpa_supplicant is running.
                        pid="$(pidof wpa_supplicant)"

                        if [ -z "${pid}" ]; then
				# Stop dhcpcd.
				dhcpcd_stop "${DEVICE}"
			fi
		fi

		if [ -n "${PPTP_ROUTE}" ]; then
			route del ${PPTP_ROUTE}
		fi

		if [ "$DEVICE" != "${GREEN_DEV}" ] && [ "$DEVICE" != "" ]; then
			link_status=`ip link show $DEVICE.${INET_VLAN} 2> /dev/null`
			if [ -n "${link_status}" ]; then
				if echo "${link_status}" | grep -q UP; then
					boot_mesg "Bringing down the ${DEVICE}.${INET_VLAN} interface..."
					ip link set ${DEVICE}.${INET_VLAN} down
					vconfig rem ${DEVICE}.${INET_VLAN}
					evaluate_retval
				fi
			else
				link_status=`ip link show $DEVICE 2> /dev/null`
				if [ -n "${link_status}" ]; then
					if echo "${link_status}" | grep -q UP; then
						boot_mesg "Bringing down the ${DEVICE} interface..."
						ip link set ${DEVICE} down
						evaluate_retval
					fi
				fi
			fi
		fi
		killall -w -s KILL /usr/sbin/pppd >/dev/null 2>&1
		killall -w -s KILL pptp >/dev/null 2>&1
		killall -w -s KILL br2684ctl >/dev/null 2>&1

		exit 0;
		;;
esac
