#!/bin/sh
########################################################################
# Begin $rc_base/init.d/leds
#
# Description : Script to setup leds at boot.
#
########################################################################

. /etc/sysconfig/rc
. ${rc_functions}

if [ -e /etc/init.d/leds.user ]; then
	/etc/init.d/leds.user $*
	exit ${?}
fi

# Load ethernet settings
eval $(/usr/local/bin/readhash /var/ipfire/ethernet/settings)

case "${RED_TYPE}" in
	PPPOE)
		RED_DEV="ppp0"
		;;
esac

# setup_netdev_trigger LED DEVICE MODE
setup_netdev_trigger ()
{
	if [ -d "/sys/class/leds/$1" ]; then
		modprobe -q ledtrig-netdev 2>&1 > /dev/null
		echo "netdev" > /sys/class/leds/$1/trigger
		echo "$2" >     /sys/class/leds/$1/device_name
		echo "$3 $4" >  /sys/class/leds/$1/mode
	fi
}

# setup_netdev_trigger LED
setup_heartbeat_trigger ()
{
	if [ -d "/sys/class/leds/$1" ]; then
		modprobe -q ledtrig-heartbeat 2>&1 > /dev/null
		echo "heartbeat" >  /sys/class/leds/$1/trigger
	fi
}

# disable_led_trigger LED
disable_led_trigger ()
{
	if [ -d "/sys/class/leds/$1" ]; then
		echo "none" >     /sys/class/leds/$1/trigger
		echo "0" >        /sys/class/leds/$1/brightness
	fi
}

# enable LED
enable_led ()
{
	if [ -d "/sys/class/leds/$1" ]; then
		echo "1" >        /sys/class/leds/$1/brightness
	fi
}

case "${1}" in
	start)
		# Alix LED start
		setup_heartbeat_trigger alix:1
		setup_netdev_trigger alix:2 ${RED_DEV} rx
		setup_netdev_trigger alix:3 ${RED_DEV} tx

		# Apu LED start
		setup_heartbeat_trigger apu:1
		setup_netdev_trigger apu:2 ${RED_DEV} rx
		setup_netdev_trigger apu:3 ${RED_DEV} tx

		# Geos LED start
		setup_heartbeat_trigger geos:1
		setup_netdev_trigger geos:2 ${RED_DEV} rx
		setup_netdev_trigger geos:3 ${RED_DEV} tx

		# Dreamplug
		setup_netdev_trigger dreamplug:green:wifi ${GREEN_DEV} tx rx
		setup_netdev_trigger dreamplug:green:wifi_ap ${BLUE_DEV} tx rx
		setup_netdev_trigger dreamplug:blue:bluetooth ${RED_DEV} tx rx

		# Iomega iConnect start
		setup_heartbeat_trigger iconnect:blue:otb
		setup_netdev_trigger iconnect:blue:power ${RED_DEV} rx
		setup_netdev_trigger iconnect:red:power ${RED_DEV} tx
		setup_netdev_trigger iconnect:blue:usb_2 ${GREEN_DEV} tx rx
		setup_netdev_trigger iconnect:blue:usb_3 ${BLUE_DEV} tx rx
		setup_netdev_trigger iconnect:blue:usb_4 ${ORANGE_DEV} tx rx

		# ICY Box LED start
		setup_netdev_trigger nas6210:red:power ${RED_DEV} tx rx
		setup_netdev_trigger nas6210:red:usb_copy ${GREEN_DEV} tx rx

		# Mirabox start
		setup_heartbeat_trigger mirabox:green:pwr
		setup_netdev_trigger mirabox:green:stat ${GREEN_DEV} tx rx
		setup_netdev_trigger mirabox:blue:stat ${BLUE_DEV} tx rx

		# Nanopi R1 start
		setup_heartbeat_trigger nanopi-r1:red:status
		setup_netdev_trigger nanopi-r1:green:wan ${RED_DEV} tx rx
		setup_netdev_trigger nanopi-r1:green:lan ${GREEN_DEV} tx rx

		exit 0
	;;

	stop)
		# Alix LED stop
		disable_led_trigger alix:1
		enable_led alix:1
		disable_led_trigger alix:2
		disable_led_trigger alix:3

		# Apu LED stop
		disable_led_trigger apu:1
		enable_led apu:1
		disable_led_trigger apu:2
		disable_led_trigger apu:3

		# Geos LED stop
		disable_led_trigger geos:1
		enable_led geos:1
		disable_led_trigger geos:2
		disable_led_trigger geos:3

		# Dreamplug
		disable_led_trigger dreamplug:green:wifi
		disable_led_trigger dreamplug:green:wifi_ap
		disable_led_trigger dreamplug:blue:bluetooth

		# Iomega iConnect stop (heartbeat will leave on)
		disable_led_trigger iconnect:blue:power
		disable_led_trigger iconnect:red:power
		disable_led_trigger iconnect:blue:usb_2
		disable_led_trigger iconnect:blue:usb_3
		disable_led_trigger iconnect:blue:usb_4

		# ICY Box LED stop
		disable_led_trigger nas6210:red:power
		disable_led_trigger nas6210:red:usb_copy

		# Mirabox stop
		disable_led_trigger mirabox:green:pwr
		enable_led mirabox:green:pwr
		disable_led_trigger mirabox:green:stat
		disable_led_trigger mirabox:blue:stat

		# Nanopi R1 stop
		disable_led_trigger nanopi-r1:red:status
		enable_led nanopi-r1:red:status
		disable_led_trigger nanopi-r1:green:wan
		disable_led_trigger nanopi-r1:green:lan

		exit 0
	;;

	*)
		echo "Usage: ${0} {start|stop}"
		exit 1
	;;
esac

# End $rc_base/init.d/leds
