--- a/drivers/pci/quirks.c	2008-09-08 20:33:16.000000000 +0200
+++ b/drivers/pci/quirks.c	2008-09-11 08:52:32.000000000 +0200
@@ -1381,6 +1381,50 @@
 			 PCI_DEVICE_ID_TOSHIBA_TC86C001_IDE,
 			 quirk_tc86c001_ide);
 
+/*
+ * The Twinhad H12Y assign mmio (0xffbfe800-0xffbfecff)
+ * resources that seems to be used by an unknown device.
+ * This quirk reserve more than really used mmio space to
+ * force change the mmio area of the cardreader and the network chip.
+ * See http://bugzilla.kerbel.org/show_bug.cgi?id=10231
+ * and http://bugzilla.kerbel.org/show_bug.cgi?id=9905
+ * for more details
+ */
+static void __init quirk_h12y_1_mmio(struct pci_dev *dev)
+{
+/*
+ * Network Device: Realtek 8139C of Twinhead H12Y
+ * PCI VENDOR: 0x10EC PCI ID:0x8139
+ * SUB VENDOR: 0x14FF SUB ID:0xA003
+ */
+	struct resource *r = &dev->resource[1];
+	if ((dev->subsystem_vendor) == 0x14FF &&
+	    (dev->subsystem_device) == 0xA003) {
+		r->start = 0;
+		r->end = 0x03ff;
+	}	
+}
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_REALTEK,
+			PCI_DEVICE_ID_REALTEK_8139,
+			quirk_h12y_1_mmio);
+
+static void __init quirk_h12y_2_mmio(struct pci_dev *dev)
+{
+/*
+ * SD-Cardreader Device: O2 7120 of Twinhead H12Y
+ * PCI VENDOR: 0x1217 PCI ID:0x7120
+ * SUB VENDOR: 0x14FF SUB ID:0xA003
+ */
+	struct resource *r = &dev->resource[0];
+	if ((dev->subsystem_vendor) == 0x14FF &&
+	    (dev->subsystem_device) == 0xA003) {
+		r->start = 0;
+		r->end = 0x03ff;
+	}	
+}
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_O2,0x7120,quirk_h12y_2_mmio);
+
+
 static void __devinit quirk_netmos(struct pci_dev *dev)
 {
 	unsigned int num_parallel = (dev->subsystem_device & 0xf0) >> 4;
